	2024 ASBESTOS REGISTER – GRANT (Building 11), Rockhampton Girls Grammar School  
Date of register: 05/08/2024
NOTE: A demolition or refurbishment survey should be carried out by a competent person before undertaking refurbishment or demolition work.

	Workplace address:
	Rockhampton Girls 
Grammar School –
Denham Street, 
Rockhampton City QLD 4700
	Name and contact details of competent person:
	Lawrence Lyons
Asbestos Assessor Licence No. 2317266

Environics (QLD) Pty Ltd
ABN 76 354 368 913
Tel. 0429 128 145

	Workplace owner / manager:
	Kasey Mitchell
Facilities and Services Manager Rockhampton Girls Grammar School 
Tel. 0427 414 819

	Areas not assessed:
	Ceiling cavities located beyond inspection openings, utility pits, and elevated areas where safety measures cannot be practically implemented.

	Asbestos related 
documents:
	ENV-2023-062  Ver 1-4 Asbestos Management Plan & ACM Register - RGGS, Denham St The Range Q 4700.pdf   
· Appendix One	ENV-2023-062-RGGS-ASBESTOS REGISTER-v1-02.10.2024. (this document)
· Appendix Two         RGGS-691-PRO-ASBESTOS-MANAGEMENT-PROCEDURE-v1-24.07.2024
· Appendix Three      RGGS-692-PRO-ASBESTOS-INCIDENT-MANAGEMENT-PROCEDURE-v1-24.07.2024
· Appendix Four       RGGS-720-GDL-ASBESTOS-MANAGEMENT-POSTER-v1-24.07.2024


	Consultation:
	Attach minutes of relevant future meeting to this document.

	Disclaimer and 
Limitations:
	Inspections were limited to accessible areas without dismantling or removing objects, including vegetation, insulation, coverings, furnishings, and personal belongings. Areas such as inside walls, between floors, and behind stored items were not inspected. No destructive procedures were performed, and relevant legislation was followed. For further details on regulations, please refer to additional materials. Compliance and Liability: This register does not serve as a 'Certificate of Compliance' unless specified and does not warranty against future asbestos issues. The report does not confirm that all areas are asbestos-free. The competent person is not liable for undetectable asbestos requiring structural disruption. 

	

Date
	
Sample       No.
	Type of material identified or assumed and amount 
(Cross-sectional areas
 are estimates – measure before quoting)
	
Friable or non-friable asbestos
	

Condition of asbestos
	
Specific location of identified or assumed asbestos
	


Notes

	05/08/2024
	
ENV001
	
Chrysotile 
>40m2
	
Non-friable unless removed using an abrasive method of removal i.e. lift & grinding concrete

 
	
Fair condition with an area of cracked tiles at center of room
	
Interior:
Vinyl floor tiles to the Art room below the G1class room
	
COHLABS Certificate of Analysis 24-9180
Recommend removed during 2025 due to area of poor condition at center of room. 

	 05/08/2024
	
  G5
	
Chrysotile >50m2
	

 Non-friable
	
Fair 
	Internal wall & ceiling sheeting to the fire escape stairwell on the southern side of the building 
	    19 October 2013 – SLR report:
A number of asbestos labels were sighted



. 
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	2024 ASBESTOS REGISTER – GRANT (Building 11), Rockhampton Girls Grammar School  
NOTE: A demolition or refurbishment survey should be carried out by a competent person before undertaking refurbishment or demolition work.

	NON-ASBESTOS MATERIALS

The following materials were tested and found not to contain asbestos:


	Date 
	  Sample
No.
	Result of Analysis
	Location 
	Notes

	
05/08/2024
	
P7
	No Asbestos fibre detected
	Exterior:
External ceiling sheeting to the covered walkway off the Dining-Lounge-Laundry 
	19 October 2013 – SLR report:


	
05/08/2024
	
P8
	     No Asbestos detected.

	Exterior:
Fibrous sheeting to the ground floor sunshades located to the building - Fibrous sheeting to the level 1 sunshades located to the building
	19 October 2013 – SLR report:
Sampling of ground floor sunshades on western side of building do not contain asbestos. No access to sunshades on north, east and south sides of building - presumed to contain asbestos.

	
	
	
	The desktop review of historical records, including Asbestos Removal Control Plans (ARCPs), Asbestos Clearance Certificates, and additional documentation, coupled with the walkthrough inspection, verified that asbestos-containing materials (ACMs) have been removed and that modern renovations have taken place. 
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	Vinyl tiles containing asbestos 
	Area were cracking of tiles has occurred
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	Asbestos cement wall sheeting – stairwell southern end of building  
	Asbestos cement ceiling sheeting – stairwell southern end of building  
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