	2024 ASBESTOS REGISTER – HERITAGE PLAYSHED (Building 17), Rockhampton Girls Grammar School  
Date of register: 06/06/2024
NOTE: A demolition or refurbishment survey should be carried out by a competent person before undertaking refurbishment or demolition work.

	Workplace address:
	Rockhampton Girls 
Grammar School –
Denham Street, 
Rockhampton City QLD 4700
	Name and contact details of competent person:
	Lawrence Lyons
Asbestos Assessor Licence No. 2317266

Environics (QLD) Pty Ltd
ABN 76 354 368 913
Tel. 0429 128 145

	Workplace owner / manager:
	Kasey Mitchell
Facilities and Services Manager Rockhampton Girls Grammar School 
Tel. 0427 414 819

	Areas not assessed:
	Ceiling cavities located beyond inspection openings, utility pits, and elevated areas where safety measures cannot be practically implemented.

	Asbestos related 
documents:
	ENV-2023-062  Ver 1-4 Asbestos Management Plan & ACM Register - RGGS, Denham St The Range Q 4700.pdf   
· Appendix One	ENV-2023-062-RGGS-ASBESTOS REGISTER-v1-02.10.2024. (this document)
· Appendix Two         RGGS-691-PRO-ASBESTOS-MANAGEMENT-PROCEDURE-v1-24.07.2024
· Appendix Three      RGGS-692-PRO-ASBESTOS-INCIDENT-MANAGEMENT-PROCEDURE-v1-24.07.2024
· Appendix Four       RGGS-720-GDL-ASBESTOS-MANAGEMENT-POSTER-v1-24.07.2024


	Consultation:
	Attach minutes of relevant future meeting to this document.

	Disclaimer and 
Limitations:
	Inspections were limited to accessible areas without dismantling or removing objects, including vegetation, insulation, coverings, furnishings, and personal belongings. Areas such as inside walls, between floors, and behind stored items were not inspected. No destructive procedures were performed, and relevant legislation was followed. For further details on regulations, please refer to additional materials. Compliance and Liability: This register does not serve as a 'Certificate of Compliance' unless specified and does not warranty against future asbestos issues. The report does not confirm that all areas are asbestos-free. The competent person is not liable for undetectable asbestos requiring structural disruption. 

	

Date
	
Sample       No.
	Type of material identified or assumed and amount 
(Cross-sectional areas
 are estimates – measure before quoting)
	
Friable or non-friable asbestos
	

Condition of asbestos
	
Specific location of identified or assumed asbestos
	


Notes

	
10/04/2024
	
 PF1
	
Chrysotile 24m2
	

Non-friable unless removed by abrasive means, i.e. floor grind after lifting
	
Fair
	
Interior:
Storerooms 5, 6, 7 & 8
	
19 October 2013 – SLR report:

Vinyl floor tiles to the storerooms 5, 6, 7 & 8 along with the Stationery Store - Chrysotile Asbestos fibre detected.

	  
  10/04/2024
	
PF2
	Chrysotile
65 to 85 m2
	

Non-friable 
	
Poor to Fair
	Interior:
Walls of storerooms and room 8, walls for former shop, canteen & dressing rooms. Partition walls between rooms. Infill panel on north wall in north eastern closed storage, second hand clothes room, all outer walls to store rooms
	19 October 2013 – SLR report:

Rep sample of internal wall sheeting to storeroom, room no. 8 - Chrysotile Asbestos fibre detected the sheeting to storerooms, uniform shop, canteen & dressing rooms, walls and partition walls run up and to the beginning of the ceiling cavity. 
Several walls were found to be plaster or canite.
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Date
	
Sample       No.
	Type of material identified or assumed and amount 
(Cross-sectional areas
 are estimates – measure before quoting)
	
Friable or non-friable asbestos
	

Condition of asbestos
	
Specific location of identified or assumed asbestos
	


Notes

	
10/04/2024
	
 PF4

	
Chrysotile
120 m2
	
Non-Friable
	
Fair

	Exterior:
Wall sheeting and cover strips of building 

	      19 October 2013 – SLR report:
External wall sheeting and cover strips to the Building - Chrysotile Asbestos fibre detected

	10/04/2024
	 S14
	Chrysotile
12 m2
	
Non-Friable
	
Fair

	Interior:
Wall of western elevation of main room
	  Sampled during the 2024 inspections. 

	10/04/2024
	 S15
	Chrysotile
12 m2
	
Non-Friable
	
Fair

	Interior:
Wall adjacent to north entry to building
	  Sampled during the 2024 inspections. 
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Photo 1 Location of Sample 14.

Photo 2 Location o Sample 15

The residual asbestos sheeting is a bonded (non-friable) materials that is painted. The overallrisk rating for
the building is low.




