	2024 ASBESTOS REGISTER – JACKSON HOUSE (Building 24), Rockhampton Girls Grammar School  
Date of register: 06/06/2024
NOTE: A demolition or refurbishment survey should be carried out by a competent person before undertaking refurbishment or demolition work.

	Workplace address:
	Rockhampton Girls 
Grammar School –
Denham Street, 
Rockhampton City QLD 4700
	Name and contact details of competent person:
	Lawrence Lyons
Asbestos Assessor Licence No. 2317266

Environics (QLD) Pty Ltd
ABN 76 354 368 913
Tel. 0429 128 145

	Workplace owner / manager:
	Kasey Mitchell
Facilities and Services Manager Rockhampton Girls Grammar School 
Tel. 0427 414 819

	Areas not assessed:
	Ceiling cavities located beyond inspection openings, utility pits, and elevated areas where safety measures cannot be practically implemented.

	Asbestos related 
documents:
	ENV-2023-062  Ver 1-4 Asbestos Management Plan & ACM Register - RGGS, Denham St The Range Q 4700.pdf   
· Appendix One	ENV-2023-062-RGGS-ASBESTOS REGISTER-v1-02.10.2024. (this document)
· Appendix Two         RGGS-691-PRO-ASBESTOS-MANAGEMENT-PROCEDURE-v1-24.07.2024
· Appendix Three      RGGS-692-PRO-ASBESTOS-INCIDENT-MANAGEMENT-PROCEDURE-v1-24.07.2024
· Appendix Four       RGGS-720-GDL-ASBESTOS-MANAGEMENT-POSTER-v1-24.07.2024


	Consultation:
	Attach minutes of relevant future meeting to this document.

	Disclaimer and 
Limitations:
	Inspections were limited to accessible areas without dismantling or removing objects, including vegetation, insulation, coverings, furnishings, and personal belongings. Areas such as inside walls, between floors, and behind stored items were not inspected. No destructive procedures were performed, and relevant legislation was followed. For further details on regulations, please refer to additional materials. Compliance and Liability: This register does not serve as a 'Certificate of Compliance' unless specified and does not warranty against future asbestos issues. The report does not confirm that all areas are asbestos-free. The competent person is not liable for undetectable asbestos requiring structural disruption. 

	

Date
	
Sample       No.
	Type of material identified or assumed and amount 
(Cross-sectional areas
 are estimates – measure before quoting)
	
Friable or non-friable asbestos
	

Condition of asbestos
	
Specific location of identified or assumed asbestos
	


Notes

	09/04/2024
	 S11

	Chrysotile
>30m2
[bookmark: _GoBack]
	Non-friable unless removed using an abrasive method of removal i.e. lift & grinding concrete


	
Fair 
	
Interior:
Vinyl floor tiles of the fire escape stairwell at the northern end of the building
	
Walls and ceiling sheeting in same area, no asbestos detected

	09/04/2024
	
-
	Presumed 
Chrysotile
>30m2

	
Non-friable 

	Fair 

	
Exterior:
Upper most level – Soffits 
	
Unable to access due to working at height restriction. Material of same appearance tested at Luck Building and found to contain Chrysotile asbestos.  



. 
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	2024 ASBESTOS REGISTER – FLORENCE HOUSE, Rockhampton Girls Grammar School  
Date of register: 06/06/2024
NOTE: A demolition or refurbishment survey should be carried out by a competent person before undertaking refurbishment or demolition work.

	NON-ASBESTOS MATERIALS

The following materials were tested and found not to contain asbestos:


	Date 
	  Sample
No.
	Result of Analysis
	Location 
	Notes

	09/04/2024
	S04
	 No Asbestos Detected
	Exterior:
Ground floor ceiling of open covered area adjacent to library on the western side of the building
	COHLABS Certificate of Analysis 
No. 24-4489
Extensive modern renovations have occurred in this area

	09/04/2024
	S07
	 No Asbestos Detected
	Exterior:
Compressed cement sheeting attached to uncover stairwell infrastructure 
	COHLABS Certificate of Analysis 
No. 24-4489


	09/04/2024
	S08
	 No Asbestos Detected
	Interior:
Wall sheeting within fire cabinet on level one, hallway west  
	COHLABS Certificate of Analysis 
No. 24-4489. 


	09/04/2024
	S09
	 No Asbestos Detected
	Interior:
 Wall sheeting within fire cabinet on level one, hallway east  
	COHLABS Certificate of Analysis 
No. 24-4489. 

	09/04/2024
	S10
	 No Asbestos Detected
	Interior:
 Wall sheeting storeroom on level one
	COHLABS Certificate of Analysis 
No. 24-4489.  Some Synthetic mineral fibres (SMF) detected in sample

	09/04/2024
	S12
	 No Asbestos Detected
	Interior:
 Wall sheeting within fire escape stairwell, at northern end of building  
	COHLABS Certificate of Analysis 
No. 24-4489. 

	09/04/2024
	S13
	 No Asbestos Detected
	Interior:
 Ceiling sheeting within fire escape stairwell, at northern end of building  
	COHLABS Certificate of Analysis 
No. 24-4489.
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Photo 1 - Soffit of Upper Level - Presumed Asbestos Based on Testing Elsewhere
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