	2024 ASBESTOS REGISTER –McKeague Hall (Building ##), Rockhampton Girls Grammar School  
Date of register: 10/04/2024
NOTE: A demolition or refurbishment survey should be carried out by a competent person before undertaking refurbishment or demolition work.

	Workplace address:
	Rockhampton Girls 
Grammar School –
Denham Street, 
Rockhampton City QLD 4700
	Name and contact details of competent person:
	Lawrence Lyons
Asbestos Assessor Licence No. 2317266

Environics (QLD) Pty Ltd
ABN 76 354 368 913
Tel. 0429 128 145

	Workplace owner / manager:
	Kasey Mitchell
Facilities and Services Manager Rockhampton Girls Grammar School 
Tel. 0427 414 819

	Areas not assessed:
	Ceiling cavities located beyond inspection openings, utility pits, and elevated areas where safety measures cannot be practically implemented.

	Asbestos related 
documents:
	ENV-2023-062  Ver 1-4 Asbestos Management Plan & ACM Register - RGGS, Denham St The Range Q 4700.pdf   
· Appendix One	ENV-2023-062-RGGS-ASBESTOS REGISTER-v1-02.10.2024. (this document)
· Appendix Two         RGGS-691-PRO-ASBESTOS-MANAGEMENT-PROCEDURE-v1-24.07.2024
· Appendix Three      RGGS-692-PRO-ASBESTOS-INCIDENT-MANAGEMENT-PROCEDURE-v1-24.07.2024
· Appendix Four       RGGS-720-GDL-ASBESTOS-MANAGEMENT-POSTER-v1-24.07.2024


	Consultation:
	Attach minutes of relevant future meeting to this document.

	Disclaimer and 
Limitations:
	Inspections were limited to accessible areas without dismantling or removing objects, including vegetation, insulation, coverings, furnishings, and personal belongings. Areas such as inside walls, between floors, and behind stored items were not inspected. No destructive procedures were performed, and relevant legislation was followed. For further details on regulations, please refer to additional materials. Compliance and Liability: This register does not serve as a 'Certificate of Compliance' unless specified and does not warranty against future asbestos issues. The report does not confirm that all areas are asbestos-free. The competent person is not liable for undetectable asbestos requiring structural disruption. 

	

Date
	
Sample       No.
	Type of material identified or assumed and amount 
(Cross-sectional areas
 are estimates – measure before quoting)
	
Friable or non-friable asbestos
	

Condition of asbestos
	
Specific location of identified or assumed asbestos
	


Notes

	
10/04/2024
	
M5
	
Chrysotile & Amosite
	
Non-friable

	Fair condition 

	
Interior:
Storage cupboard located below the stairwell at the entry to the Hall – Wall and Ceiling Sheets
	
SLR reported dated 19/10/2013

	
14/09/2024
	
002 – same as Luck building
	
Chrysotile, Amosite, & Crocidolite 
	

Non-friable 
	
Good – Painted 
	
Exterior:
Level One - External cover sheeting of column sampled at edge
	
Fibre cement material – COHLABS Certificate No. 24-10941

	
14/09/2024
	
003 same as Luck building
	
Chrysotile & Amosite 
	

Non-friable 
	
Good – Painted 
	
Exterior:
Level One - External cover molding over cladding 
	
Fibre cement material – COHLABS Certificate No. 24-10941



. 
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	2024 ASBESTOS REGISTER – LUCK (Building 10), Rockhampton Girls Grammar School  
Date of register: 29/10/2024
NOTE: A demolition or refurbishment survey should be carried out by a competent person before undertaking refurbishment or demolition work.

	

Date
	
Sample       No.
	Type of material identified or assumed and amount 
(Cross-sectional areas
 are estimates – measure before quoting)
	
Friable or non-friable asbestos
	

Condition of asbestos
	
Specific location of identified or assumed asbestos
	


Notes

	
14/09/2024
	
004
same as Luck building
	
Chrysotile, Amosite, & Crocidolite 
	

Non-friable 
	
Good – Painted 
	
Exterior:
Level One - External cover molding over cladding 
	
Fibre cement material – COHLABS Certificate No. 24-10941

	
14/09/2024
	
005
same as Luck building
	
Chrysotile & Amosite 
	

Non-friable 
	
Good – Painted 
	
Exterior:
Level One - External infill panel above window 
	
Fibre cement material – COHLABS Certificate No. 24-10941

	
14/09/2024
	
006
same as Luck building
	
Chrysotile & Amosite 
	

Non-friable 
	
Good – Painted 
	
Exterior:
Level One - External cover flat molding above window 
	
Fibre cement material – COHLABS Certificate No. 24-10941
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